7.2. Following Protocol Streams
Prev | Chapter 7. Advanced Topics | Next

## 7.2. Following Protocol Streams

It can be very helpful to see a protocol in the way that the application layer sees it. Perhaps you are looking for passwords in a Telnet stream, or you are trying to make sense of a data stream. Maybe you just need a display filter to show only the packets in a TLS or SSL stream. If so, Wireshark’s ability to follow protocol streams will be useful to you.

To filter to a particular stream, select a packet in the packet list of the stream/connection you are interested in and then select the menu item you want under Analyze → Follow (or in the context menu in the packet list). Wireshark will set an appropriate display filter and display a dialog box with the data from the stream laid out, as shown in Figure 7.1, “The “Follow TCP Stream” dialog box”.

| Tip
Following a protocol stream applies a display filter which selects all the packets in the current stream. Some people open the “Follow TCP Stream” dialog and immediately close it as a quick way to isolate a particular stream. Closing the dialog with the “Back” button will reset the display filter if this behavior is not desired.

Wireshark supports following the streams of many different protocols, including TCP, UDP, DCCP, TLS, HTTP, HTTP/2, QUIC, WebSocket, SIP, and USB CDC. The dialog for following TCP streams is covered in detail here; most other supported protocols will show dialogs which are very similar.

| Note
If the type of stream you wish to follow is disabled or missing from the menu, Wireshark did not find the respective protocol in the currently selected packet.

| Tip
To follow TLS or SSL streams, see the wiki page on TLS for instructions on providing TLS keys.

Figure 7.1. The “Follow TCP Stream” dialog box

The stream content is displayed in the same sequence as it appeared on the network. Non-printable characters are replaced by dots. Traffic from the client to the server is colored red, while traffic from the server to the client is colored blue. These colors can be changed by opening Edit → Preferences and under Appearance → Font and Colors, selecting different colors for the Sample "Follow Stream" client text and Sample "Follow Stream" server text options.

The stream content won’t be updated while doing a live capture. To get the latest content you’ll have to reopen the dialog.

You can choose from the following actions:

Help
  Show this help.
Filter out this stream
  Apply a display filter removing the current stream data from the display.
Print
  Print the stream data in the currently selected format.
Save as…​
  Save the stream data in the currently selected format.
Back
  Close this dialog box and restore the previous display filter.
Close
  Close this dialog box, leaving the current display filter in effect.

By default, Wireshark displays both client and server data. You can select the Entire conversation to switch between both, client to server, or server to client data.

You can choose to view the data in one of the following formats:

ASCII
  In this view you see the data from each direction in ASCII. Obviously best for ASCII based protocols, e.g., HTTP.
C Arrays
  This allows you to import the stream data into your own C program.
EBCDIC
  For the big-iron freaks out there.
HEX Dump
  This allows you to see all the data. This will require a lot of screen space and is best used with binary protocols.
UTF-8
  Like ASCII, but decode the data as UTF-8.
UTF-16
  Like ASCII, but decode the data as UTF-16.
YAML
  This allows you to load the stream as YAML.

The YAML output is divided into 2 main sections:

- The `peers` section where for each `peer` you found the peer index, the `host` address and the `port` number.
- The `packets` section where for each `packet` you found the packet number in the original capture, the `peer` index, the packet `index` for this peer, the `timestamp` in seconds and the `data` in base64 encoding.

Example 7.1. Follow Stream YAML output

    peers:
      - peer: 0
        host: 127.0.0.1
        port: 54048
      - peer: 1
        host: 127.0.10.1
        port: 5000
    packets:
      - packet: 1
        peer: 0
        index: 0
        timestamp: 1599485409.693955274
        data: !!binary |
          aGVsbG8K
      - packet: 3
        peer: 1
        index: 0
        timestamp: 1599485423.885866692
        data: !!binary |
          Ym9uam91cgo=

The same example but in old YAML format (before version 3.5):

    # Packet 1
    peer0_0: !!binary |
      aGVsbG8K
    # Packet 3
    peer1_0: !!binary |
      Ym9uam91cgo=

How the old format data can be found in the new format:

New YAML format | Old YAML format |
--- | --- | ---
    ...
    packets:
      - packet: AAA
        peer: BBB
        index: CCC
        data: !!binary |
          DDD
    # Packet AAA
    peerBBB_CCC !!binary |
      DDD
    AAA: packet number in the original capture
    BBB: peer index
    CCC: packet index for this peer
    DDD: data in base64 encoding

Raw
  This allows you to load the unaltered stream data into a different program for further examination. The display will show the data as strings of hex characters with each frame on a separate line, but “Save As” will result in a binary file without any added line separators.

You can optionally show the delta time each time the direction changes (turns) or for every packet or event.

You can switch between streams using the “Stream” selector.

You can search for text by entering it in the “Find” entry box and pressing Find Next.

Figure 7.2. The “Follow HTTP/2 Stream” dialog box

The HTTP/2 Stream dialog is similar to the "Follow TCP Stream" dialog, except for an additional "Substream" dialog field. HTTP/2 Streams are identified by a HTTP/2 Stream Index (field name `http2.streamid`) which are unique within a TCP connection. The “Stream” selector determines the TCP connection whereas the “Substream” selector is used to pick the HTTP/2 Stream ID.

The QUIC protocol is similar, the first number selects the QUIC connection number while the "Substream" field selects the QUIC Stream ID.

Figure 7.3. The “Follow SIP Call” dialog box

The SIP call is shown with same dialog, just filter is based on sip.Call-ID field. Count of streams is fixed to 0 and the field is disabled.

Prev | Up | Next
Chapter 7. Advanced Topics | Home | 7.3. Show Packet Bytes